|  |  |  |
| --- | --- | --- |
| Diagram  Description automatically generated with medium confidence | **Staunton Harold Sailability Trust** |  |

**Hereford Hoist user instructions**

**A metal pole on a dock

AI-generated content may be incorrect.**

**Safe operation requires two people**

1. The hoist must be located in the mounting provided on the pontoon, check it is secure and rotate the hoist arm fully to check free movement.
2. Check the hanger attachment is fitted correctly on the end of the arm.
3. Check the piston ensuring it is clean and free of dirt and there are no oil leaks.
4. The arm is raised and lowered by hydraulic pressure, there is a valve on the cylinder that controls the speed of lowering, and a handle that pumps up the pressure raising the arm.
5. To lower the arm, release the valve by turning anti clockwise till you arrive at the desired height then close by turning clockwise to finger tight.
6. To raise the arm the valve must be closed then using the handle pump the arm up till it reaches the desired height, only raise it to the height required.
7. To move the hoist into the correct position for lifting or lowering rotate the whole hoist by pushing using the hoist arm.
8. When using the sling ensure that it is fully around the person being lifted and cross the handles before attaching to the hoist handle.
9. Before lifting put tension on the sling attachments by raising the hoist arm, check by pulling that these are secure before continuing.
10. Raise the person until at the desired height over the pontoon before swinging them over to the boat.
11. Once in position over the seat in the boat slowly lower the arm until the person is located in the seat.
12. Once in position remove the sling attachment from the hoist raise and move out of the way.
13. Leave the sling in place around the person so its ready to recover them when they return.